**Quotes for the wetpour repair needed at the junior swings**

3 companies quoted.

* Caloo did not include a quote for the total replacement. Let’s assume it would be proportionate but I’ll ask them to give me one, hopefully in time for Tuesday
* Redlynch quoted very late so I am pursuing the query about ‘overlaying’ with them and can update you at the meeting

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Company** | **Area repair** | **Full replacement** | **Notes on guarantee** | **Other notes** |
| Redlynch | £1,100 | £2,581 | 3 years on full repair but very limited on the area repair | Calls the full replacement an overlay not removal and disposal (cf Vitaplay) |
| Vitaplay | £569 | £2,914 | queried | Offered edge repairs at £427. There is a gap |
| Caloo | £545 | Assume competitive with Vitaplay but requested | Same as Redlynch |  |

From Redlynch Leisure

Liz,

Our ref 2309094

We've called in to inspect the damaged surface.  It is possible to repair it, but we couldn't offer a guarantee with the work, as   a repair might split from the original surface at some time in the future.  The cost of the repair would be £1100.00

Alternatively, it would be possible to overlay the surface with a new layer of wet pour rubber.  The cost of that would be £2581.00, and the work would be guaranteed for three years.

Prices exclude VAT.

From Vitaplay

Dear Liz,

Thank you for the opportunity to provide you with a quotation for the flat swing surface reairs at Rectory Road Recreation Ground, please find associated costs as follows:

**Option One - Repair**

* Removal and disposal of approx 4.5m2 EPDM (Clean cut across the bottom edge, removing the whole damaged area
* Supply and installation of 4,5m2 black EPDM with green fleck

**Subtotal: £568.80 VAT £113.76 Total: £682.56**

**Optional Edge Repairs**

* Supply and installation of edge repairs totalling 14 linear metres x 100mm.
* Black EPDM with green fleck

**Subtotal: £427.00 VAT £85.40 Total: £512.40**

**Option Two – Full replacement**

* Removal and disposal of approx 21m2 existing EPDM
* Regrade subbase
* Supply and installation of approx 21m2 black EPDM with green fleck

**Subtotal: £2,914.40 VAT £582.88 Total: £3,497.28**

**From Caloo**

**Wetpour Repairs**

**Qty Code Unit Description Price Total**

**Discount Total Price**

1.00 T1 EA **Wetpour Repairs**

Wetpour repairs to include the removal of the

damaged wetpour, totalling a maximum of 4 SQM in

black.

£545.00 £545.00

**Sub Total** £545.00

**Project**

**Discount** £0.00

**Total Net**

**Amount** £545.00

**Total Tax**

**Amount** £109.00

Subject to Caloo Conditions of Sale

Current Manufacturing Lead Time To be confirmed at time of order

Caloo engineer to make repairs to damaged wetpour.

**Quotation**

**Total** £654.00

Liz Holland 28.9.23